**FIREROLL A0 MANUAL ROLLER SHUTTERS**

**SPECIFICATION 3-6-1**

**Fire Resistance**

Tested to IMO Resolution A.754 (18) for 60 minutes, rated A0 and approved by most major marine authorities.

**Curtain**

Constructed from 51mm flat galvanised steel laths with steel endlocks fitted to alternate laths to prevent lateral movement. The bottom rail is a reinforced lath for uniformity of appearance.

**Guides**

The side guides are formed from galvanised steel channels and prepared for fixing to the opening structure by means of continuous fixing angles.

**Endplates**

Fabricated from galvanised steel of adequate thickness relative to door size and supplied with angles for fixing to the structure.

**Roller**

The roller is manufactured from mild steel tube of sufficient diameter and wall thickness to resist deflection and is mounted in cups on each end plate. A galvanised steel casing is supplied as standard.

**Finish**

Galvanised as standard. They are also available in grade 304 or 316 stainless steel or polyester powder coated in a range of standard RAL colours at extra cost.

**Weight**

Approximately 25 kgs per m².

**Operation**

Manual operation (push up, pull down).

**Fire Activation**

In a fire condition, closure is effected by a local fusible link which releases a drop bar. If remote activation is required from the fire alarm system or the bridge, a 24 or 220 volt DC magnet is available at extra cost.

**To specify state:**

**Fireroll A0 Fire Resisting Roller Shutters shall be by**

**Bolton Gate Company, Waterloo Street, Bolton BL1 2SP, UK Tel: 01204 871001**

**E-mail:** **sales@boltongate.co.uk** **Web:** [**www.boltongate.co.uk**](http://www.boltongate.co.uk)

**Issue Date: April 2018**